Skip to main content
`Ctrl`+`K`
scipy.signal.

# lp2lp_zpk

scipy.signal.lp2lp_zpk(z, p, k, wo=1.0)

  Transform a lowpass filter prototype to a different frequency.

  Return an analog low-pass filter with cutoff frequency wo from an analog low-pass filter prototype with unity cutoff frequency, using zeros, poles, and gain (‘zpk’) representation.

  Parameters:
    z array_like

      Zeros of the analog filter transfer function.

    p array_like

      Poles of the analog filter transfer function.

    k float

      System gain of the analog filter transfer function.

    wo float

      Desired cutoff, as angular frequency (e.g., rad/s). Defaults to no change.

  Returns:
    z ndarray

      Zeros of the transformed low-pass filter transfer function.

    p ndarray

      Poles of the transformed low-pass filter transfer function.

    k float

      System gain of the transformed low-pass filter.

  See also

  `lp2hp_zpk`, `lp2bp_zpk`, `lp2bs_zpk`, `bilinear`
  `lp2lp`

  Notes

  This is derived from the s-plane substitution

  \[s \rightarrow \frac{s}{\omega_0}\]

  Added in version 1.1.0.

  Examples

  Use the ‘zpk’ (Zero-Pole-Gain) representation of a lowpass filter to transform it to a new ‘zpk’ representation associated with a cutoff frequency wo.

      >>> from scipy.signal import lp2lp_zpk
      >>> z   = [7,   2]
      >>> p   = [5,   13]
      >>> k   = 0.8
      >>> wo  = 0.4
      >>> lp2lp_zpk(z, p, k, wo)
      (   array([2.8, 0.8]), array([2. , 5.2]), 0.8)